When sensor value is from 0 to 100, my led should glow 30%.

When value is 400, it should glow 10%.

900-1001, it should glow Max.

1001-….., TURN OFF.

Serial.write(“..”);

Serial.print(“…”);

Serial.println(“..”);

**HOME AUTOMATION:**

NAME: SAHILPATEL

PASSWORD: VIDHIISCHHOTU

PORT NO.: 1110